{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["CDKOHSL","工程量清单"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"CDKOHSL","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}

{"sheet":"工程量清单","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"merged":[[0,0,0,7],[7,0,7,1]]}
["工程量清单"]
["标段编号：SBLW",{"$nulls":6},"货币单位：人民币元"]
["段落","劳务分包项目","单 位","数 量","最高限价单价\n(不含税)","投标报价\n单价\n(不含税)","投标报价\n合价\n(不含税)","备注"]
["K120-K225、K226-K329","PCR改性乳化沥青粘层","m2",537368.85,0.35,null,{"$f":"IF(F4>E4,\"报价无效\",F4*D4)","v":0},"包含所有机械及油、人工"]
["K120-K225","ES-2型稀浆封层","m2",548610,{"v":1.2,"d":"1.20"},null,{"$f":"IF(F5>E5,\"报价无效\",F5*D5)","v":0},"包含所有机械及油、人工"]
["K226-K329","同步碎石封层","m2",410475,{"v":1.2,"d":"1.20"},null,{"$f":"IF(F6>E6,\"报价无效\",F6*D6)","v":0},"包含所有机械及油、人工"]
["K120-K225、K226-K329","PC-2乳化沥青透层","m2",956835,0.35,null,{"$f":"IF(F7>E7,\"报价无效\",F7*D7)","v":0},"包含所有机械及油、人工"]
["投标报价合计  人民币(元)",{"$nulls":5},{"$f":"SUM(G4:G7)","v":0}]