{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["CDKOHSL","工程量清单"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"CDKOHSL","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}

{"sheet":"工程量清单","index":1,"n_rows":38,"n_cols":7,"rows_kept":38,"merged":[[0,0,0,6],[36,0,36,5],[37,0,37,6]]}
["G110线K555+000-K564+600段公路养护工程招标\n工程量清单"]
[{"$nulls":6},"货币单位：人民币元"]
["序号","项目名称","单位","工程量","最高限价单价\n(不含税)","投标单价      （不含税）","投标报价\n(不含税)"]
[1,"挖除沥青混凝土路面","m3",284.31,27,null,{"$f":"IF(F4>E4,\"报价无效\",D4*F4)","v":0}]
[2,"挖除水泥稳定碎石基层","m3",3640.19,27,null,{"$f":"IF(F5>E5,\"报价无效\",D5*F5)","v":0}]
[3,"铣刨水泥混凝土路面","m3",37.1,141,null,0]
[4,"铣刨沥青混凝土路面","m3",1675.85,26,null,0]
[5,"挖土方","m3",757.7,5,null,0]
[6,"回填铣刨料","m3",3677.6,9,null,0]
[7,"借土填方","m3",636.7,9,null,0]
[8,"垫层-过渡三角区","m3",462,9,null,0]
[9,"水泥稳定级配碎石基层-厚200mm","m2",47685,43,null,0]
[10,"水泥稳定级配碎石基层-过渡三角区、找平层","m3",88,226,null,0]
[11,"C20水泥混凝土基层","m3",1023.71,339,null,0]
[12,"PC-2乳化沥青透层","m2",48223,3.8,null,0]
[13,"PCR改性乳化沥青粘层","m2",44909.6,{"v":1.5,"d":"1.50"},null,0]
[14,"ES-2型烯浆封层","m2",47685,6.5,null,0]
[15,"中粒式改性沥青混合料路面-40mm","m2",95980.1,22,null,0]
[16,"中粒式改性沥青混合料路面-沥青混凝土过渡、找平层","m3",28.2,525,null,0]
[17,"砂砾培路肩","m3",1197.7,11,null,0]
[18,"现浇混凝土加固土路肩-C20混凝土","m3",73.5,492,null,0]
[19,"沥青路面拉毛","m2",69130.6,1.5,null,0]
[20,"路面灌缝","m",23034.4,7.5,null,0]
[21,"防撞墙栏杆涂漆","m",385,7,null,0]
[22,"防撞墙防腐涂层","m2",451,21,null,0]
[23,"Gr-A-4E","m",3498,316,null,0]
[24,"AT1-2","个",17,5354,null,0]
[25,"BT-1-1","个",19,4875,null,0]
[26,"防撞桶","个",34,242,null,0]
[27,"道口标柱","个",72,70,null,0]
[28,"热熔反光标线","m2",4393.2,35,null,0]
[29,"振动热熔反光标线","m2",1701,95,null,0]
[30,"VG-De（Rbw）-E","个",291,51,null,0]
[31,"VG-De（Rbw）-At1","个",82,5,null,0]
[32,"VG-De（Rbw）-At2","个",30,5,null,0]
[33,"立面标记","m2",200,202,null,0]
["合计总金额 ",{"$nulls":5},{"$f":"SUM(G4:G36)","v":0}]
["注： 1、路面摊铺机械使用要求：福格勒2100-3L、天顺长城1860等机型。\n        2、水稳摊铺机械使用要求：天顺长城1660／1860、沃尔沃8820、徐工1253T/953T、三一C8系列等机型。\n        3、压路机系列使用要求：戴纳派克6200+宝马203+悍马138等机型。\n        4、其他要求：\n          （1）保险：施工单位给项目施工人员上雇主责任险（24小时）。\n          （2）特种作业人员必须持有特种人员证书，特种设备操作证。\n          （3）资金拨付情况由业主拨款后再向乙方支付。"]