{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["CDKOHSL","工程量清单"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"CDKOHSL","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}

{"sheet":"工程量清单","index":1,"n_rows":13,"n_cols":8,"rows_kept":13,"merged":[[0,0,0,7],[12,0,12,1]]}
["工程量清单"]
["标段编号：TP-1",{"$nulls":6},"货币单位：人民币元"]
["段落","劳务分包项目","单 位","数 量","最高限价单价\n(不含税)","投标报价\n单价\n(不含税)","投标报价\n合价\n(不含税)","备注"]
["K120-K225、K226-K329","4cm改性AC-16摊铺","m2",666160,2.3,null,{"$f":"IF(F4>E4,\"报价无效\",F4*D4)","v":0},"包含摊铺、碾压、成型、清扫的所有人工，机械"]
["K120-K225、K226-K329","5cm改性AC-16摊铺","m2",80190,{"v":2.3,"d":"2.30"},null,0,"包含摊铺、碾压、成型、清扫的所有人工，机械"]
["K120-K225","铣刨4cm原沥青面层","m3",10985.496,{"v":28,"d":"28.00"},null,0,"包含铣刨及清扫的所有人工、机械"]
["K226-K329","铣刨3cm原沥青面层","m3",2622.375,{"v":28,"d":"28.00"},null,0,"包含铣刨及清扫的所有人工、机械"]
["K226-K329","铣刨7cm原沥青面层","m3",14287.875,{"v":28,"d":"28.00"},null,0,"包含铣刨及清扫的所有人工、机械"]
["K226-K329","水泥混凝土路面拉毛","m2",1125,{"v":1.3,"d":"1.30"},null,0,"包含拉毛及清扫的所有人工、机械"]
["K120-K225","沥青路面拉毛","m2",187132.5,{"v":1.3,"d":"1.30"},null,0,"包含拉毛及清扫的所有人工、机械"]
["K226-K329","挖除旧路20cm水稳基层","m3",2738.2,15.66,null,0,"包含挖除及清扫的所有人工、机械"]
["K226-K329","挖除旧路24cm水稳基层","m3",17.856,15.66,null,0,"包含挖除及清扫的所有人工、机械"]
["投标报价合计  人民币(元)",{"$nulls":5},{"$f":"SUM(G4:G12)","v":0}]